**DISH CABLE INSTRUCTIONS FOR RECEIVING HD SIGNAL**

Please make sure the TV is hooked into the coax on the wall outlets. You will also need to perform a channel scan on the TV to pull in the Channels. (See details Below)

Channel Scan for TV.

All TVs are different and will have different functions, but please follow these main steps.

1. On your TV make sure your input is on TV.

2. Go to TV Menu or Settings

3. Go to >Channels >Program > **Cable** or Air > Auto Program

4. Please make sure settings is set to Cable (**NOT AIR**).

5. Then perform an Auto Scan. This will scan all channels and program to your TV.

If unable to use these instructions and still have trouble, you may need to look up the manufacturer for that TV and perform a Channel Search.